# Android fstab file.
# The filesystem that contains the filesystem checker binary (typically /system) cannot
# specify MF_CHECK, and must come before any filesystems that do specify MF_CHECK

# NOTE: /vendor partition is now early-mounted and the fstab entry is specified in device tree (duplicated below for recovery image purposes only):
#       /proc/device-tree/firmware/android/fstab/vendor

#TODO: Add 'check' as fs_mgr_flags with data partition.
# Currently we dont have e2fsck compiled. So fs check would failed.

# Non-A/B fstab.qcom variant
#<src>                                                              <mnt_point>            <type>  <mnt_flags and options>                                                                           <fs_mgr_flags>
/dev/block/zram0                                                    none                   swap    defaults                                                                                          zramsize=50%,max_comp_streams=8,zram_backingdev_size=512M
/dev/block/bootdevice/by-name/system                                /                      ext4    ro,barrier=1,discard                                                                              wait,avb
/dev/block/bootdevice/by-name/userdata                              /data                  ext4    nosuid,nodev,barrier=1,discard,noauto_da_alloc,noatime,lazytime                                   wait,check,formattable,fileencryption=ice,quota,reservedsize=128M
/dev/block/bootdevice/by-name/misc                                  /misc                  emmc    defaults                                                                                          defaults
/dev/block/bootdevice/by-name/modem                                 /vendor/firmware_mnt   vfat    ro,shortname=lower,uid=1000,gid=1000,dmask=227,fmask=337,context=u:object_r:firmware_file:s0      wait
/dev/block/bootdevice/by-name/bluetooth                             /vendor/bt_firmware    vfat    ro,shortname=lower,uid=1002,gid=3002,dmask=227,fmask=337,context=u:object_r:bt_firmware_file:s0   wait
/dev/block/bootdevice/by-name/dsp                                   /vendor/dsp            ext4    ro,nosuid,nodev,barrier=1                                                                         wait
/dev/block/bootdevice/by-name/cache                                 /cache                 ext4    nosuid,nodev,barrier=1,noauto_da_alloc,discard,noatime,lazytime                                   wait
/dev/block/bootdevice/by-name/cache                                 /cache                 f2fs    nosuid,nodev,fsync_mode=nobarrier,discard,noatime,lazytime                               	     wait
/dev/block/bootdevice/by-name/persist                               /mnt/vendor/persist    ext4    nosuid,nodev,barrier=1,noatime                                                                    wait
/dev/block/bootdevice/by-name/vendor                                /vendor                ext4    ro,barrier=1                                                                                      wait,recoveryonly
/dev/block/bootdevice/by-name/boot                                  /boot                  emmc    defaults                                                                                          defaults
/dev/block/bootdevice/by-name/recovery                              /recovery              emmc    defaults                                                                                          recoveryonly
/devices/platform/soc/a800000.ssusb/a800000.dwc3/xhci-hcd.0.auto*   /storage/usbotg        vfat    nosuid,nodev                                                                                      wait,voldmanaged=usbotg:auto
/devices/platform/soc/c084000.sdhci/mmc_host*                       /storage/sdcard1       vfat    nosuid,nodev                                                                                      wait,voldmanaged=sdcard1:auto,encryptable=userdata
