# Android fstab file.
# The filesystem that contains the filesystem checker binary (typically /system) cannot
# specify MF_CHECK, and must come before any filesystems that do specify MF_CHECK

#TODO: Add 'check' as fs_mgr_flags with data partition.
# Currently we dont have e2fsck compiled. So fs check would failed.

# A/B fstab.qcom variant
#<src>                                                      <mnt_point>           <type>  <mnt_flags and options>                                                                             <fs_mgr_flags>
/dev/block/zram0                                            none                  swap    defaults                                                                                            zramsize=2415919104,max_comp_streams=8
/dev/block/bootdevice/by-name/system                        /                     ext4    ro,barrier=1,discard                                                                                wait,slotselect,verify
/dev/block/bootdevice/by-name/userdata                      /data                 ext4    nosuid,nodev,barrier=0,noauto_da_alloc,discard,noatime,lazytime                                     wait,resize,check,crashcheck,quota,fileencryption=ice
/dev/block/bootdevice/by-name/userdata                      /data                 f2fs    nodev,noatime,nosuid,inline_xattr,reserve_root=32768,resgid=1065,background_gc=on                   wait,resize,check,crashcheck,quota,fileencryption=ice
/dev/block/bootdevice/by-name/misc                          /misc                 emmc    defaults                                                                                            defaults
/dev/block/bootdevice/by-name/modem                         /vendor/firmware_mnt  vfat    ro,shortname=lower,uid=1000,gid=1000,dmask=227,fmask=337,context=u:object_r:firmware_file:s0        wait,slotselect
/dev/block/bootdevice/by-name/bluetooth                     /vendor/bt_firmware   vfat    ro,shortname=lower,uid=1002,gid=3002,dmask=227,fmask=337,context=u:object_r:bt_firmware_file:s0     wait,slotselect
/devices/soc/a800000.ssusb/a800000.dwc3/xhci-hcd.0.auto*    /storage/usbotg       vfat    nosuid,nodev                                                                                        wait,voldmanaged=usbotg:auto
/dev/block/bootdevice/by-name/dsp                           /vendor/dsp           ext4    ro,nosuid,nodev,barrier=1                                                                           wait,slotselect
/dev/block/bootdevice/by-name/persist                       /mnt/vendor/persist   ext4    nosuid,nodev,barrier=1,noatime                                                                      wait,check
